li.right#macro-dropdown
	a.menu-button(href="#")
		+navbar_led("hid-recorder-led", "led-gear")
		span Macro

	.menu
		.text
			b Record and play HID/ATX/GPIO actions#[br]
			sub For security reasons, the record will not be saved on the PiKVM
		hr

		.buttons.buttons-row
			button.row25#hid-recorder-record(disabled data-force-hide-menu) &bull; Rec
			button.row25#hid-recorder-stop(disabled) Stop
			button.row25#hid-recorder-play(disabled) Play
			button.row25#hid-recorder-clear(disabled) Clear
		hr

		table.kv
			tr
				td Script time:
				td.value#hid-recorder-time(colspan="2") 00:00:00.0
			tr
				td Scripted events:
				td.value#hid-recorder-events-count 0
				td #[sup #[i include delays]]
		hr

		+menu_switch_table("hid-recorder-loop-switch", false, false) Infinite loop playback:
		hr

		input#hid-recorder-new-script-file(type="file" style="display: none")

		.buttons.buttons-row
			button.row50#hid-recorder-upload(disabled) Upload script
			button.row50#hid-recorder-download(disabled) Download script
